Modeling Tutorials > Using Photos to Model Façades >
Add Detail to the Arch

The arch is the distinctive feature of Facade4. It calls for more complex modeling than the doorways of the previous façade.

Set up the lesson:

- Continue working from the previous lesson.

Add edges for the arch:

The window edges give you a starting point, but to model the arch well, you need to add some further edges for reference and for making cuts.

1. Pan and zoom so you have a good view of the arch.
2. On the ribbon Edit panel, turn on (SwiftLoop) again.
3. Add a horizontal loop at the top of the arch.
4. Add a vertical loop at each side of the arch.
5. Subdivide the arch area with four horizontal loops. Make them a little closer together at the top, and more widely spaced toward the bottom.
6. Add one more horizontal loop for the doorstep or sidewalk.
7. Subdivide the arch area further with vertical loops: Add two on the left, and three on the right.

Outline the arch:

1. On the ribbon Edit panel, turn on (Cut).
2. Cut edges to define the archway.

   Reminder: Don’t click the mouse when the cursor shows it’s on a face. The cuts should always join edges or vertices.

3. Right-click to close the Cut tool.
4. If you want to adjust the cuts, turn on (Vertex), then move the new vertices in X or Y (try not to deform the horizontal and vertical lines of the grid).

When the cuts for the archway are done, you’re ready to extrude the arch.

Extrude the arch:

1. On the ribbon, click (Polygon) to go to the Polygon sub-object level.
2. Click and Ctrl+click to select the faces in the archway. Don’t neglect the small triangular faces that you might have created along the upper edge of the arch.
3. Drag the left edge of the ViewCube so the view shows some depth.
4. On the ribbon Polygons panel, Shift+click (Extrude) to display the extrusion caddy.

   You will extrude the arch in two stages: The first stage gives depth to the wall, and the second represents part of the interior of the arcade behind the arch.

5. In the caddy’s Height field, enter –0.3m for the first extrusion (the width of the wall).
6. Instead of clicking OK, click (Apply And Continue).

   3ds Max Design creates the extrusion and begins another.

7. In the Height field, enter –0.4 for the second extrusion (the arcade interior).
8. Click (OK) to accept the value and close the caddy.

Next

Add Detail to the Cornice