Inputting and Outputting Media > Supported Media Files Formats > Export Formats >

# Export: Supported MXF OP-1a File Codecs

Smoke supports the export of MXF OP-1a files (including the timecode) encoded with audio encoded as PCM, 16-Bit or 24-Bit, using any of the following codecs.

CODEC | Comment
--- | ---
AVC-Intra 50 |
AVC-Intra 100 |
DVCPRO |
DVCPRO 50 NTSC |
DVCPRO 50 PAL |
DVCPRO HD | Available in 1080p@25/50, 1080p@24/30/60, 720p@25/50, and 720p@24/30/60.
DNxHD | The application can export to all the timings and resolutions supported for DNxHD import.
MPEG HD422 | XDCAM HD 422 media Only available for source clips @ PAL timings.