Inputting and Outputting Media > Clip Output Using Real-Time Deliverables >

# Real-Time Deliverables Timing Specifications

When you set up a Deliverable to modify the timing of a clip during real-time output, the timing is changed according to the following tables.

NoteIn the following tables, N/A stands for not applicable and NC stands for no change in timing.

Destination timings 23.967psf through 25p:

Source |  |  |  |  | Destination |  |  |
--- | --- | --- | --- | --- | --- | --- | --- | ---
| 23.967psf | 23.967p | 24psf | 24p | PAL | 50i | 25psf | 25p
23.967psf | N/A | NC | Speed up | Speed up | Speed up to 25 or speed up to 24 + PAL Pulldown | Speed up | Speed up | Speed up
23.967p | NC | N/A | Speed up | Speed up | Speed up to 25 or speed up to 24 + PAL Pulldown | Speed up | Speed up | Speed up
24psf | Slow down | Slow down | N/A | NC | Speed up to 25 or apply PAL Pulldown | Speed up | Speed up | Speed up
24p | Slow down | Slow down | NC | N/A | Speed up to 25 or apply PAL Pulldown | Speed up | Speed up | Speed up
PAL | Slow down | Slow down | Slow down | Slow down | N/A | NC | NC | NC
50i | Slow down | Slow down | Slow down | Slow down | NC | N/A | NC | NC
25psf | Slow down | Slow down | Slow down | Slow down | NC | NC | N/A | NC
25p | Slow down | Slow down | Slow down | Slow down | NC | NC | NC | N/A

NoteWhen going from 23.967 to PAL, you can choose between increasing the frame rate to 25 or increasing to 24 and adding PAL Pulldown. When going from 24 to PAL, you can choose between increasing the frame rate to 25 or adding PAL Pulldown.

Destination timings NTSC through 60p:

Source |  |  |  |  | Destination |  |
--- | --- | --- | --- | --- | --- | --- | ---
| NTSC | 29.97p | 30 psf | 30p | 60i | 59.94p | 60p
23.967psf | Add Pulldown | Not supported | Not supported | Not supported | Speed up to 24 + Add Pulldown | Not supported | Not supported
23.967p | Add Pulldown | Not supported | Not supported | Not supported | Speed up to 24 + Add Pulldown | Not supported | Not supported
24psf | Slow Down to 23.976 + Add Pulldown | Not supported | Not supported | Not supported | Add Pulldown | Not supported | Not supported
24p | Slow Down to 23.976 + Add Pulldown | Not supported | Not supported | Not supported | Add Pulldown | Not supported | Not supported
PAL | Slow Down to 23.976 + Add Pulldown | Not supported | Not supported | Not supported | Slow Down to 24 + Add Pulldown | Not supported | Not supported
50i | Slow Down to 23.976 + Add Pulldown | Not supported | Not supported | Not supported | Slow Down to 24 + Add Pulldown | Not supported | Not supported
25psf | Slow Down to 23.976 + Add Pulldown | Not supported | Not supported | Not supported | Slow Down to 24 + Add Pulldown | Not supported | Not supported
25p | Slow Down to 23.976 + Add Pulldown | Not supported | Not supported | Not supported | Slow Down to 24 + Add Pulldown | Not supported | Not supported
NTSC | N/A | NC | Speed up | Speed up | Speed up | Not supported | Not supported
29.97p | NC | N/A | Speed up | Speed up | Speed up | Not supported | Not supported
30 psf | Slow down | Slow down | N/A | NC | NC | Not supported | Not supported
30p | Slow down | Slow down | NC | N/A | NC | Not supported | Not supported
60i | Slow down | Slow down | NC | Field merge | N/A | Not supported | Not supported
59.94p | Not supported | Not supported | Not supported | Not supported | Not supported | N/A | Speed up
60p | Not supported | Not supported | Not supported | Not supported | Not supported | Slow down | N/A