Inputting and Outputting Media > Clip Input/Output Using a VTR >

# Outputting Clips To a VTR

Once you have clips that are ready for output to tape, you can use the Output Clip menu to perform this operation. Like capturing, you can output single clips or multiple clips, and enable a split view to preview the clip you want to output alongside the media on the tape simultaneously.

Another way to output multiple clips is to generate an EDL and then output the clips using the EDL.

Most of the procedures in this section assume that you have already blacked your tape. However, if necessary, you can output in assemble mode, which allows you to perform clip output to a tape that was only partially blacked. See Outputting Clips in Assemble Mode.

For HD-specific considerations, see Supported HD Formats for Video I/O.

#### Topics in this section

- Accessing the Output Clip Menu
- Output Clip Menu Controls
- Selecting a VTR Device For Output
- Outputting a Single Clip
- Outputting Multiple Clips
- Outputting Clips With a Letterbox Overlay
- Outputting Clips with a Logo Overlay
- Outputting Clips in Assemble Mode
- HDCAM SR Stereo Tape Output