Inputting and Outputting Media > Supported Media Files Formats > Import Formats >

# Import: Supported Audio File Formats

Smoke supports import and soft-import of the following audio file formats.

Files of any sample rate can be imported, but they are all resampled to 48 kHz.

NoteThe Import Image menu can soft-import only a limited set of audio file formats: AIFF, AIFF-C, and WAVE. The Gateway library method has no such limitation. See Importing Media Files.

File Format | Default Extension | Bit Depth
--- | --- | ---
AIFF-C | aifc | 16, 24, or 32 (float)
AIFF | aiff | 16 or 24
Nextsnd | au | 16, 24, or 32 (float)
MP3 | mp3 | 16
WAVE | wav | 16, 24, or 32 (float)
Broadcast Wave | wav | 16, 24, or 32 (float)
Berkeley/IRCAM/CARL Sound (BISCF) | bsf | 16
Audio Visual Research | avr | 16