Inputting and Outputting Media > Clip Input/Output Using HSDL Devices >

# Setting Up Hardware for HSDL Input and Output

Connect the HSDL device using the same method for serial dual RGB 4:4:4 video I/O. To control the HSDL device remotely, connect the device using an RS-422 cable to the serial port on the workstation that corresponds to the port defined in the software initialisation configuration file. See the Autodesk Visual Effects and Finishing Configuration File Reference Guide.