Wiretap Central > Monitoring the Decoding Jobs > Understanding the Monitor User Interface >

# Servers Tab

The following table presents the information found on the Servers tab.

Column | Description
--- | ---
Name | Server name (host name)
Description | A short description of the server, entered when the server was installed
Status | The current activity of the server: absent: Server is no longer seen by the manager, possibly down. active: Server is currently working on a job. suspended: Server has been put on hold. idle: Server is inactive. error: Server is experiencing a problem.
Perf. Index | A value in the range [0–1] indicating the performance level of the server, relative to other servers on the same job. A score of 1 indicates this is the best-performing server.
Adapters | A comma-separated list of installed plug-ins and adapters, for example: Burn: The Burn renderer. Command Line Tool: The Backburner cmdjob command-line plug-in allows you to submit batch, executable, or script files to Backburner as “custom” jobs. mio: The MIO adapter is the processing engine responsible for carrying out transcoding jobs. Wire: Installed with Stone and Wire. Can be used to import/export media, perform Wire transfers, etc. Used by the Wiretap SDK’s background I/O tool, wiretap_bgio_tool.