Inputting and Outputting Media > Clip Output Using Real-Time Deliverables >

# Accessing the Deliverables Menu

Use the Deliverables menu to manage Real-Time Deliverables, and to configure real-time operations such as resize, pulldown, and so on. Many of these settings can also be altered in the Output Clip menu.

To access the Deliverables menu:

1. Select the clip you want to work on and open the Player.
2. Click the Deliverables tab.

   The Deliverables menu appears.

   (a) Source clip information(b) Resize and frame rate controls(c) Audio controls (d) LUT controls(e) Stereo controls(f) Letterbox controls(g) Deliverable controls(h) Deliverable box

Most of the controls in the Deliverables menu are common to various parts of the software, and their functions are explained in their respective sections. The following does not describe how to use the controls, but rather how to manage the results using Deliverables and output them to tape in real time. The settings you create in the Deliverables menu can be previewed in the Player and are applied in real time during clip output.

To configure real-time operations, see Managing Deliverables.

NoteSettings in the Deliverables menu override clip settings from other modules. These settings are overridden, not discarded. For example, if a Deliverable has LUTs set, the LUTs from the source clip are not used.

Source clip information
  Displays information about the source clip before real-time operations are applied.
Resize controls
  Displays values set in the Resize editor, accessible with the Editor button. You can edit the values directly in the Deliverables menu. The available destination resolutions and timings depend on the format of the source material.
Audio controls
  Displays the audio speed. To preserve audio pitch, enable Preserve Pitch. See About the Audio Timewarp Options.
LUT controls (3D and 1D)
  Enables or disables the use of LUTs. You can specify a 3D LUT to use, and access the LUT editor.
Stereo controls
  Enables stereoscopic output settings, if a stereo track is detected. You can select a Stereo Mode option and a corresponding Method option.

Select: | To:
--- | ---
Anaglyph | Output the left eye and right eye as a red/cyan clip. You can reduce ghosting (Dubois), remove RGB values (Mono) or create custom anaglyph results.
Interlaced | Output the left eye and right eye as an interlaced RGB clip. You can output the left eye as field 1 or field 2.
Dual Image - Scale | Output the left eye and right eye so that they are adjacent to each other in the same clip, either in a left and right or top and bottom orientation.
Dual Image - Splice | Ouput the left eye and right eye so that they are side by side in the same clip. Only available when each eye track's horizontal resolution is half that of the output resolution (2 tracks at 960 for a 1920 output).
Dual Output | Output the left and right eye separately to dual streams of a tape.

Letterbox controls
  Enables or disables a letterbox overlay. See Outputting Clips With a Letterbox Overlay .
Start TC field
  Set the start timecode of the Deliverable. The start timecode is used during output, it indicates where on the tape the clip is recorded.