Procedural Compositing with Batch > Batch: Node Reference >

# MUX Node

The MUX (multiplexer) node allows you to make multiple output sockets. Use this node to propagate an input to multiple other nodes through the schematic and to clarify its graphical representation. Additionally, use the MUX node to clarify the connection scheme of nodes within a group.

Default display of MUX node input and output links

MUX node with hidden output links

In the MUX Node menu, two toggle buttons control the display of connections to and from the node.

Input button
  Enable to hide the input link to the MUX node.
Output button
  Enable to hide all output links from the MUX node.

The following are the Range settings for the MUX node:

Range Active button
  Enable to activate the range settings.
Range from field
  Displays the beginning of the range of frames that will be impacted by the MUX node
Range to field
  Displays the end of the range of frames that will be impacted by the MUX node.
Range before button
  Enable to select between Repeat First, No Media, Use Black, and Use White. Applied before the set frame range.
Range after button
  Enable to select between Repeat First, No Media, Use Black, and Use White. Applied after the set frame range.