- Main Page
- Related Pages
- Modules
- Classes
- Examples

- Class List
- Class Hierarchy
- Class Members

Public Member Functions

# MDeviceState Class Reference
OpenMayaUI - API module for user interface

Search for all occurrences

## Detailed Description

Input device state.

MDeviceState is a generic event class for input devices. Input device classes (such as MPxMidiInputDevice) are responsible for converting specific event types to an MDeviceState which Maya understands.

Examples:

  jlcVcrDevice.cpp.

`#include <MDeviceState.h>`

List of all members.

## Public Member Functions
virtual | ~MDeviceState ()
| Class destructor.
int | devicePosition (const unsigned short int axis) const
| Returns the position of the device for the specified axis.
int | devicePosition (const MString &axisName) const
| Returns the position of the device for the specified axis.
void | setDevicePosition (const int position, const unsigned short int axis)
| Sets the position of the device for the specified axis.
void | setDevicePosition (const int position, const MString &axisName)
| Sets the position of the device for the specified axis.
bool | buttonState (const unsigned short int button) const
| Returns the state of the given button.
bool | buttonState (const MString &buttonName) const
| Returns the state of the named button.
void | setButtonState (const bool state, const unsigned short int button)
| Set the state of the specified button.
void | setButtonState (const bool state, const MString &buttonName)
| Set the state of the specified button.
int | maxAxis () const
| Return the value of the axis with the largest value.
bool | isNull ()
| Returns true if this device state is NULL;.

## Member Function Documentation

int devicePosition | ( | const unsigned short int | axis | ) | const

Search for all occurrences

Returns the position of the device for the specified axis.

Parameters:

  [in] | axis | The device axis to be tested

Returns:
  The position of the device for the specified axis

int devicePosition | ( | const MString & | axisName | ) | const

Search for all occurrences

Returns the position of the device for the specified axis.

Parameters:

  [in] | axisName | The name of the device axis to be tested

Returns:
  The position of the device for the specified axis

void setDevicePosition | ( | const int | position,
|  | const unsigned short int | axis
| ) |  |

Search for all occurrences

Sets the position of the device for the specified axis.

Parameters:

  [in] | position | The new position value
  [in] | axis | The axis of the device to be set

Examples:
  jlcVcrDevice.cpp.

void setDevicePosition | ( | const int | position,
|  | const MString & | axis
| ) |  |

Search for all occurrences

Sets the position of the device for the specified axis.

Parameters:

  [in] | position | The new position value
  [in] | axis | The name of the axis of the device to be set

bool buttonState | ( | const unsigned short int | button | ) | const

Search for all occurrences

Returns the state of the given button.

Parameters:

  [in] | button | The number of the button to be tested

Returns:
  - true button pressed
  - false button released

bool buttonState | ( | const MString & | buttonName | ) | const

Search for all occurrences

Returns the state of the named button.

Parameters:

  [in] | buttonName | The name of the button to be tested

Returns:
  - true button pressed
  - false button released

void setButtonState | ( | const bool | state,
|  | const unsigned short int | button
| ) |  |

Search for all occurrences

Set the state of the specified button.

Parameters:

  [in] | state | The state to be set (true or false)
  [in] | button | The button number

Examples:
  jlcVcrDevice.cpp.

void setButtonState | ( | const bool | state,
|  | const MString & | buttonName
| ) |  |

Search for all occurrences

Set the state of the specified button.

Parameters:

  [in] | state | The state to be set (true or false)
  [in] | buttonName | The name of the button to be set

int maxAxis | ( |  | ) | const

Search for all occurrences

Return the value of the axis with the largest value.

This is used to dejitter absolute devices.

Returns:
  The value of the largest axis

bool isNull | ( |  | ) |

Search for all occurrences

Returns true if this device state is NULL;.

Returns:
  - true The device state is NULL
  - false The device state is not NULL

Examples:
  jlcVcrDevice.cpp.

MDeviceState MDeviceState MDeviceState MDeviceState MDeviceState MDeviceState MDeviceState MDeviceState MDeviceState MDeviceState
MDeviceState MDeviceState MDeviceState MDeviceState MDeviceState MDeviceState MDeviceState MDeviceState MDeviceState MDeviceState