Reference > Properties >
Transfer Detail properties

This topic describes the options available in the Transfer Detail window. See Transfer properties between meshes and Import topology changes for workflows using these options.

Target Model

  Select the target geometry you want to transfer detail to. The ideal target mesh is a low resolution base mesh with no subdivision levels.

Source Model

  Select the source geometry and subdivision level. Select the subdivision level that most closely matches the shape of the target mesh.

  For example if you sent a level 3 mesh to Maya and want to re-import a re-topologized version of that mesh into Mudbox as the target, use a source level of 3.

Search Distance

  Sets the total distance samples can travel to find the source (high resolution) model(s). Samples can travel on both sides of the target (low resolution) model based on the Choose Samples option. Default is 4.

Advanced

Test Both Sides

  This option uses ray casting to compare the source and target meshes. The default setting is off, which means that when the ray intersects a surface that is facing in the opposite direction, the intersection is ignored. When on, Mudbox records ray intersections with source faces that are backfacing. This improves transfer results when a number of intersecting meshes are used as the source model.

Choose Samples

  Available when Method is set to Ray Casting. Determines which value to record if an extraction sample intersects the high-resolution model more than once:

Subdivide Target To

  Lets you set how many times the target mesh is subdivided during the detail transfer operation. Select from specific levels 0 through 12, or select Automatic to subdivide the target mesh to the first level with the same number of (or more) faces as the source mesh.

Select Missed Regions

  When on, any areas of the target mesh that are not transferred successfully (meaning they do not completely match the source) are selected when the transfer operation finishes. This lets you easily identify areas that may require re-sculpting.

Transfer Joint Weights

  When on, all joint weights from the source mesh are transferred to the target mesh.

  If the target mesh has existing weighting, those weights are discarded before the source weights are transferred.

  Turn off if you want to keep the existing weights on your target mesh.

Transfer Sculpt Layers

  When on, source sculpt layers are transferred to the target.

Transfer Base as Sculpt Layer

  When on, all transferred sculpt detail is placed onto a new sculpt layer for the target mesh.