Colour Correcting > About the Colour Warper > Accessing the Colour Warper >

# Accessing the Colour Warper from Modular Keyer, Action, or Paint

To access the Colour Warper from the Modular Keyer:

1. Double-click on, or drag, the Colour Warper node from the node bar to the schematic.
2. Double-click the Colour Warper node.

   You are in the Colour Warper editor.

To access the Colour Warper from Action:

1. From the Media menu, select the media containing the clip you want to colour correct.
2. Double-click the CC field for the media you want to colour warp.
3. Click the Colour box.

   The Colour box changes to CW. You are in the Colour Warper.

To access the Colour Warper from Paint:

1. Do one of the following:
   - To colour correct a clip, click Setup in the Paint menu, click CutOut, enable CC, and then enable the CC button for the clip you want to colour correct.

     The clip is loaded into the Colour Warper.

   - To colour correct a cutout, click Cut/Paste in the Paint menu, create a cutout, and then use the Colour Correction field or click CC.

     The cutout is loaded into the Colour Warper.