Importing and Exporting Media > Clip Input/Output Using a VTR > Inputting Clips From a VTR >

# Accessing the VTR Input Module

Use the VTR Input module to input clips using a VTR.

1. Select a folder from the Media Library. This is where the captured clips will be created.
2. Select File > VTR Input...

   The VTR Input module appears.

If the VTR Input... menu item is not available, it means your workstation is either not connected to a VTR, or not configured to use a VTR. In case of the former, connect a VTR to your workstation using either an AJA Io XT or an AJA Kona 3G. In case of the latter, see Configuring Software For Clip Input and Output Using a VTR