Gateway Clip Description >

# feed

The <feed> element allows you to manage and reference different qualities and resolutions for the same reference media.

Attribute | Description | Data Type | Allowed Values | Attribute is...
--- | --- | --- | --- | ---
type | The data type of the element. | character data | feed | Implied
version | Version of the xml element. Do not use, unless mixing and matching differing xml schema versions, which should not be done. | unsigned integer | 3 | Implied
vuid | Identifies the version of the feed. In a <track> element, no two <feed> elements can have the same vuid. <feed> elements in different <track> elements can share the same vuid. | ID | any unique (within <feeds>) | Required
uid | Uniquely identifies the feed within the .clip file. Duplicate uid in a .clip are not allowed. We recommend that you use a GUID, but any unique identifier will do. | ID | any unique (within .clip) | Required

Children
handler?,storageFormat?,sampleRate?,startTimecode?,startOffset?,userData?,comment?,spans

Found in...
<feeds>