Preferences >

# LUT Preferences

1D LUT/3D LUT and Colour Transform list
  Displays the list of imported 1D LUTs or 3D LUTs and Colour Transforms in separate tabs. See Making 1D LUTs Available for Display and Making 3D LUTs and Colour Transforms Available for Display.

LUT Type box
  Select whether you want to define a gamma function or import a ID LUT file in the highlighted row and assign the corresponding keyboard shortcut.

Import button
  Opens the Import LUT browser. Navigate to the 1D LUT file to import, and select it to load it into the list. This button is available when the LUT Type box is set to LUT File.

Value field
  Displays the gamma value. This field is available when the LUT Type box is set to Gamma.

Select button
  Apply the highlighted gamma or 1D LUT to all displayed images. See Applying 1D LUTs to the Monitor.

Import button
  Opens the Import LUT browser. Navigate to the 3D LUT or Colour Transform file to import, and select it to load it to the 3D LUT and Colour Transform list.

Reset button
  Removes the highlighted item from the list.

Reset All button
  Removes all LUTs and Colour Transforms from the current list.

## SynColor

Shared Directory
  Displays the file path to the shared colour transforms directory. This is a useful location for storing transforms that can be used by other applications that use Autodesk Colour Management.
Browse
  Browse to select a different shared directory for color transforms. The path you select is used by all compatible applications on the same workstation.
Default
  Reset the shared directory to /opt/Autodesk/Synergy/SynColor/Shared/transforms.
Graphics Monitor Transform
  Specifies the CTF file that is used when the graphicsMonitor alias is referenced by another CTF file. See Configuring the Graphics Monitor Alias.
Browse
  Browse to select a different colour transform for the graphicsMonitor alias.