Importing and Exporting Media > Conform Tab Overview > Conforming an EDL >

# Conforming an EDL with VTR Recapture

NoteThe following requires that the workstation is connected to a VTR.

1. In the Conform tab, right-click the Event list and select Load New EDL.
2. From the window that appears, locate and select the EDL to import, and then click Load.

   The EDL is loaded and opened as a sequence in the timeline view of the Conform tab.

3. Right-click the event list, and select Capture All From VTR.

   The VTR module opens and cues the VTR.

4. Proceed with the recapture of the cued events.
5. Once back to the Conform tab, continue with the conform process as you would with a file-based sequence.