Stabilizing and Tracking > Selecting a Stabilizer Method >

# Removing Jitter While Keeping Overall Motion

Use the Jitter option to remove the jitter from a clip while retaining the overall motion. The Stabilizer calculates the difference between an average applied to the channel by using the current Over value and the original tracking data. Applying this curve leaves only the jitter values as keyframes. Copying these curves can also be useful if you want to extract the jitter values to apply to another clip.

The Jitter option removes jitter in a clip on both the X and Y axes simultaneously, and averages the pan over time so that it appears even. Jitter control offers more flexibility than Fixed X and Fixed Y, which remove motion in one direction only. Use Fixed X and Fixed Y in simple situations, or to produce a result quickly.

Removing jitter is a process of trial and error. Try different Over values until you find one that yields good results. As a general rule, start with a large Over value over n frames to remove slow jitter, and start with a small Over value to remove fast jitter.

To remove jitter and keep overall motion:

1. Select Tools Composite Stabilizer.

   The cursor changes to Pick Front.

2. Select the front clip.

   The cursor changes to Render Here.

3. Click on any free (or a grey) area on the workspace.

   You are now in Stabilizer.

4. Position Tracker1 over a pattern you want to stabilize.
5. To automatically remove the border at the edges of the clip, select Crop Edges from the Scaling and Shifting box.
6. Go to the reference frame, and click Analyze to generate the Shift data.
7. Click Animation to display the Channel Editor. Select the tracker number and expand the Shift folder.

   The Shift curves turn white when the Shift channel is selected.

8. Select Keyframe from the Animation Controls box, and then enter an Over value in the Curve Value field.

   (a) Animation Controls box(b) Curve option box(c) Curve Value field

9. Select Jitter from the Curve option box. If Jitter was already displayed when you entered the Over value, select it again to apply the Over value.

   The transformation is applied to the curves. The curves show the amount of motion that the Stabilizer will remove. They should wrap around the zero point and should not be entirely flat; otherwise, the Stabilizer will not remove any jitter.

10. Click Result and play the clip to determine if it is stable enough. If the clip is stable enough, click Exit. To revert to the original shift data, click Paste.
11. Repeat from step 7 with different Over values until you are satisfied with the results.

#### Related Information

- Removing Jitter with Fixed X and Fixed Y