Chroma Keying and Working with Green Screens >

# Creating a Key by Extracting a Range of Colours with the HLS, YUV, RGB and RGBCMYL Keyers

Another technique for creating a key is to extract a range of colours from the key-in clip. Use this technique for clips where the colour you are extracting contains impurities.

When you build a key by defining a colour range, you can use one of four colour models: RGB, YUV, HLS, or RGBCMYL. Each model interprets the key-in clip differently and gives a slightly different result.

After you choose a colour model, you set a range of colours to become partially transparent in the key-in clip to soften the transition between the front and back clips. This is called the softness range. All pixels in the front clip within the softness range become grey in the matte. The key should have the greatest possible softness value.

After setting the softness range, you set a range of colours to be keyed out in the key-in clip. This is called the tolerance range. All pixels in the front clip within the tolerance range become black in the matte. The tolerance range must not be too large or the edge of the composite will be too hard and the subject in the front clip will appear to be pasted into the back clip.

#### Topics in this section

- About the Different Colour Models
- Selecting a Colour Model Based Component Keyer
- Setting the Softness Range
- Setting the Tolerance Range

#### Related Information

- Chroma Keying and Working with Green Screens