Importing and Exporting Media > Clip Input/Output Using a VTR >

# Supported HD Formats for Video I/O

You can input and output clips in the following HD formats.

Format | Resolution | Scanning | Supported Frame Rates
--- | --- | --- | ---
720p | 1280 x 720 | Progressive | 25, 50, 59.94, and 60 fps, Hz
1080i | 1920 x 1080 | Interlaced | 25, 29.97, and 30 fps, Hz
1080p | 1920 x 1080 | Progressive | 23.976, 24, 25, and 30 fps, Hz
1080PsF | 1920 x 1080 | Progressive | 23.976, 24 and 25 fps, Hz