Public Attributes
tagXSI_RTS_Camera Struct Reference

## Detailed Description

The XSI_RTS_Camera structure.

Holds information about a camera. Used by the legacy tagXSI_RTS_SceneData structure which is accessed via the tagXSI_RTS_SystemParams::m_SceneData member.

See also:
  tagXSI_RTS_SystemParams::m_sCamera, IRTSExecutionState::GetCamera, Camera

`#include <XSI_rtshaders.h>`

List of all members.

## Public Attributes
float | m_mMatrix [16]
eXSI_RTS_CameraType | m_eCameraType
float | m_fRight
float | m_fLeft
float | m_fTop
float | m_fBottom
float | m_fNear
float | m_fFar
float | m_fFOV
float | m_fAspect

## Member Data Documentation

float m_mMatrix[16]

The camera matrix

eXSI_RTS_CameraType m_eCameraType

The type of camera (ortho, perspective)

float m_fRight

Frustum right

float m_fLeft

Frustum left

float m_fTop

Frustum top

float m_fBottom

Frustum bottom

float m_fNear

Near plane

float m_fFar

Far plane

float m_fFOV

Field of view

float m_fAspect

Aspect ratio

The documentation for this struct was generated from the following file:

- XSI_rtshaders.h