## NurbsSurfaceMesh.Get

### Description

Returns a complete data description of a NurbsSurfaceMesh.
Note: This method uses output arguments. C# and some scripting languages (such as JScript and PerlScript) don't support arguments passed by reference. However, there is a alternate version of this method which is considered safe to use with C#, JScript and PerlScript: NurbsSurfaceMesh.Get2.

### C# Syntax

    NurbsSurfaceMesh.Get( siNurbsFormat in_eNurbsFormat, Object& out_pvsalCount, Object& out_pvsaUVControlPoints, Object& out_pvsaNbUControlPoints, Object& out_pvsaNbVControlPoints, Object& out_pvsadUKnots, Object& out_pvsaNbUKnots, Object& out_pvsadVKnots, Object& out_pvsaNbVKnots, Object& out_pvsabUClosed, Object& out_pvsabVClosed, Object& out_pvsalUDegree, Object& out_pvsalVDegree, Object& out_pvsaeUParam, Object& out_pvsaeVParam );

### Scripting Syntax

    NurbsSurfaceMesh.Get( [NurbsFormat], [Count], [UVControlPoints], [NbUControlPoints], [NbVControlPoints], [UKnots], [NbUKnots], [VKnots], [NbVKnots], [UClosed], [VClosed], [UDegree], [VDegree], [UParam], [VParam] );

### Parameters

Parameter | Type | Description
--- | --- | ---
NurbsFormat | siNurbsFormat | Specifies how the data is formatted. Default Value: siSINurbs
Count | Long | Number of NurbsSurface in the mesh.
UVControlPoints | 3D Array | The control points are stored in a 3 dimensional array. The array is 4 * (Number of V ControlPoints) * (Number of U ControlPoints)
NbUControlPoints | Array of Longs | Specifies the number of U ControlPoints per Nurbs surface.
NbVControlPoints | Array of Longs | Specifies the number of V ControlPoints per Nurbs surface.
UKnots | Array of Doubles | An array of knot values in U direction.
NbUKnots | Array of Longs | Specifies the number of U Knots per Nurbs surface.
VKnots | Array of Doubles | An array of knot values in V direction.
NbVKnots | Array of Longs | Specifies the number of V Knots per Nurbs surface.
UClosed | Array of Boolean values | Specifies whether the Nurbs surface are closed in U direction.
VClosed | Array of Boolean values | Specifies whether the Nurbs surfaces are closed in V direction.
UDegree | Array of Longs | Degree of the Nurbs surfaces in U direction.
VDegree | Array of Longs | Degree of the Nurbs surfaces in V direction.
UParam | Array of siKnotParameterization values | The parameterization factor of the Nurbs surface in U direction.
VParam | Array of siKnotParameterization values | The parameterization factor of the Nurbs surface in V direction.

### Examples

#### VBScript Example

    set obj = activeproject.activescene.root.addgeometry( "grid", "nurbssurface" )

    obj.activeprimitive.Geometry.Get siSIFormat, _

    	count, _

    	cpoints, _

    	nupoints, _

    	nvpoints, _

    	uknots, _

    	nuknots, _

    	vknots, _

    	nvknots, _

    	uclosed, _

    	vclosed, _

    	udeg, _

    	vdeg, _

    	uparam, _

    	vparam

    activeproject.activescene.root.AddNurbsSurfaceMesh2 _

    	1, _

    	cpoints, , ,_

    	uknots, ,_

    	vknots, ,_

    	udeg, _

    	vdeg, _

    	uclosed, _

    	vclosed, _

    	uparam, _

    	vparam, _

    	siSIFormat, _

    	"MyNurbsSurface"