## extrudecompaxisop

Extrude Geometry Component

Type:
  XSI Object

Spdl File:
  %XSI_HOME%\Application\spdl\C3DExtrudeComponentAxisOp.spdl

Parameter Name | Scriptname | Description | Valid Values | Data Type | Range | UI Range
--- | --- | --- | --- | --- | --- | ---
Length | length | Length |  | Double |  | -10.0 - 10.0
Duplicate Polygons | duplicate | Duplicate the polygons instead of extruding them |  | Bool |  |
Inset Amount | inset | Interior Offset |  | Double |  | -1.0 - 1.0
Inset Locked | insetlocked | The inset is automatically calculated using the length and the angle |  | Bool |  |
Angle | insetangle | The inset is automatically calculated using the length and this angle |  | Double | -89.9 - 89.9 |
X | x | X Axis |  | Bool |  |
Y | y | Y Axis |  | Bool |  |
Z | z | Z Axis |  | Bool |  |
Frame | frame | Frame |
0 | Object
1 | Component
| Integer | 0 - 1 | 0 - 1
Merge | merge | Merge adjacent polygons and use average reference frame of components |  | Bool |  |
Maintain Orthogonality | orthogonal | Ensure that extrusion is always orthogonal to component normal |  | Bool |  |
Skirting Ratio | skirtingratio | How far along the adjoining edges to add a vertex |  | Double | 0.0 - 1.0 | 0.0 - 1.0
Subdivs | subdivs | Number of Subdivisions |  | Integer |  | 0 - 10
Type | type | Type of extrude (Poly/Edge/Vertex) |  | Integer |  |
Transform Per Subdivision | persubdiv | Apply transforms per subdiv or per extrude |  | Bool |  |
X | sx | Scale in X |  | Double |  | 0.0 - 10.0
Y | sy | Scale in Y |  | Double |  | 0.0 - 10.0
Z | sz | Scale in Z |  | Double |  | 0.0 - 10.0
X | rx | Rotation in X |  | Double |  | -180.0 - 180.0
Y | ry | Rotation in Y |  | Double |  | -180.0 - 180.0
Z | rz | Rotation in Z |  | Double |  | -180.0 - 180.0
X | tx | Translation in X |  | Double |  | -10.0 - 10.0
Y | ty | Translation in Y |  | Double |  | -10.0 - 10.0
Z | tz | Translation in Z |  | Double |  | -10.0 - 10.0
Start | start | Start |  | Double |  | 0.0 - 100.0

Autodesk Softimage v7.5