XSI_ImageFX

Stores the special effect parameters applied to the image.

All parameters are animatable. Fcurve names are:

• HUE

• GAIN

• SATURATION

• BRIGHTNESS

• BLUR_RADIUS

• BLUR_AMOUNT

• BLUR_ALPHA

• SCALING_TYPE

• SCALE-X

• SCALE-Y

• FLIP-X

• FLIP-Y

• RGBA2GRAYSCALE

• BITS_PER_CHANNEL

| This template is not available in SI|3D.

| This template corresponds to the CSLImageFX class.

Introduced

3.6

Template

    XSI_ImageFX {
       // Color Correction
       <Hue>,
       <Gain>,
       <Saturation>,
       <Brightness>,
       // Blur
       <Radius>,
       <Amount>,
       <blurAlpha>,
       // Scaling
       <type>
       <scaleX>,<scaleY>,
       // Flip
       <horizontal>,<vertical>,
       // Conversion
       <conversion>,
       <8 buts to 16 bits per channel>
           }

Members

Member name | Description
Hue | Hue color correction. Possible values are between 0 (default) and 100.
Gain | Gain color correction. Possible values are between 0 (default) and 100.
Saturation | Saturation color correction. Possible values are between 0 (default) and 100.
Brightness | Brightness color correction. Possible values are between -100 and 100 (with 0 being the default).
Radius | Radius of blur. Possible values are between 0 and 20 (with 0 being the default).
Amount | Amount of blur. Possible values are 0 or 1 (default).
blurAlpha | True to blur the Alpha channel.
type | Scaling information. Possible values are: • 0 = none (scaling is inactive) • 1 = fullsize • 2 = halfsize • 3 = quartersize • 4 = 128 X 128 • 5 = 256 X 256 • 6 = 512 X 512 • 7 = Custom (use scaleX and scaleY)
scaleX | Specify amount to scale in X (used only for Custom type of scaling).
scaleY | Specify amount to scale in Y (used only for Custom type of scaling).
horizontal | Specify horizontal flip value.
vertical | Specify vertical flip value.
conversion | Specifies whether or not to convert RGBA to greyscale. Possible values are: • 1 = True (convert RGBA to greyscale) • 0 = False (do not convert RGBA to greyscale)
16bits | Specifies whether to use 16 bits per channel or 8bits. Possible values are: • 1 = True (use 16 bits per channel) • 0 = False (use 8 bits per channel)

Example

See the example in XSI_Image.

Autodesk Softimage v7.5