## addedgeop

Add an edge between an existing point and an existing edge

Type:
  XSI Object

Spdl File:
  %XSI_HOME%\Application\spdl\C3DAddEdgeOp.spdl

Parameter Name | Scriptname | Description | Valid Values | Data Type | Range | UI Range
--- | --- | --- | --- | --- | --- | ---
Ratio Edge | ratioedge | Ratio on edge where to split to end the new edge |  | Double | 0.0 - 100.0 | 0.0 - 100.0
New Edge ID | newedgeid | ID of new edge created by the operation |  | Integer | 0 - Max |
New Point ID | newptid | ID of new point created by the operation (-1 if ratioedge = 0 or 100%) |  | Integer | 0 - Max |
New Points ID | newptsid | ID of all new points created by the operation (-1 if ratioedge = 0 or 100% with no interior point) |  | 8195 |  |

Autodesk Softimage v7.5