## loft

Loft

Type:
  XSI Object

Spdl File:
  %XSI_HOME%\Application\spdl\LoftOp.spdl

Parameter Name | Scriptname | Description | Valid Values | Data Type | Range | UI Range
--- | --- | --- | --- | --- | --- | ---
Scale Factor | startscl | Scale factor applied to continuity with start surface |  | Float | -10.0 - 10.0 | -1.0 - 1.0
Scale Factor | endscl | Scale factor applied to continuity with end surface |  | Float | -10.0 - 10.0 | -1.0 - 1.0
Continuity at Surface Curve | startcont | Continuity at surface curve of start surface |
0 | G0 (Position)
1 | G1 (Tangent)
2 | G2 (Normal)
| Integer |  |
Continuity at Surface Curve | endcont | Continuity at surface curve of end surface |
0 | G0 (Position)
1 | G1 (Tangent)
2 | G2 (Normal)
| Integer |  |
Tangent Direction Match | starttandir | Tangent direction match at start surface |  | Bool |  |
Tangent Direction Match | endtandir | Tangent direction mattch at end surface |  | Bool |  |
Curve Tolerance | crvtol | Curve tolerance applied to each curve of the loft |  | Float | 0.0 - 2.0 | 0.0 - 2.0
Position Tolerance | postol | Position tolerance of lofted surface |  | Float | 0.0 - 2.0 | 0.0 - 2.0
Angular Tolerance | angtol | Angular tolerance of lofted surface |  | Float | 0.0 - 2.0 | 0.0 - 2.0
Close in U | closeu | Close resulting surface in U |  | Bool |  |
Close in V | closev | Close resulting surface in V |  | Bool |  |

Autodesk Softimage v7.5