## upvctcns

Upvector Direction Constraint

Type:
  XSI Object

Spdl File:
  %XSI_HOME%\Application\spdl\C3DBaseUpVectorCns.spdl

Parameter Name | Scriptname | Description | Valid Values | Data Type | Range | UI Range
--- | --- | --- | --- | --- | --- | ---
Up Vector Active | upvct_active | UpVector Activeness |  | Bool |  |
Roll | roll | UpVector Roll |  | Double | Min - Max | -360.0 - 360.0
Axis to Align - Up Vector | upaxis | Axis to Align along the Up Vector |  | 0 |  |
X | upx | X Component |  | Double | Min - Max | -1.0 - 1.0
Y | upy | Y Component |  | Double | Min - Max | -1.0 - 1.0
Z | upz | Z Component |  | Double | Min - Max | -1.0 - 1.0
Point At - Up Vector | pointat | Point at offset for the up vector |  | 0 |  |
X | pointatx | Point at Offset X |  | Double | Min - Max | -10.0 - 10.0
Y | pointaty | Point at Offset Y |  | Double | Min - Max | -10.0 - 10.0
Z | pointatz | Point at Offset Z |  | Double | Min - Max | -10.0 - 10.0

Autodesk Softimage v7.5