## fillHoleOp

Type:
  XSI Object

Spdl File:
  %XSI_HOME%\Application\spdl\fillHoleOp.spdl

Parameter Name | Scriptname | Description | Valid Values | Data Type | Range | UI Range
--- | --- | --- | --- | --- | --- | ---
Side Continuity Srf 1 | SideContinuitySrf1 | Side Continuity Srf 1 |  | Integer | 0 - 2 | 0 - 2
Side Continuity Srf 2 | SideContinuitySrf2 | Side Continuity Srf 2 |  | Integer | 0 - 2 | 0 - 2
Side Continuity Srf 3 | SideContinuitySrf3 | Side Continuity Srf 3 |  | Integer | 0 - 2 | 0 - 2
Side Continuity Srf 4 | SideContinuitySrf4 | Side Continuity Srf 4 |  | Integer | 0 - 2 | 0 - 2
Side Continuity Srf 5 | SideContinuitySrf5 | Side Continuity Srf 5 |  | Integer | 0 - 2 | 0 - 2
Inter Boundary Continuity 1 | InterBoundaryContinuity1 | Inter Boundary Continuity 1 |  | Integer | 0 - 2 | 0 - 2
Inter Boundary Continuity 2 | InterBoundaryContinuity2 | Inter Boundary Continuity 2 |  | Integer | 0 - 2 | 0 - 2
Inter Boundary Continuity 3 | InterBoundaryContinuity3 | Inter Boundary Continuity 3 |  | Integer | 0 - 2 | 0 - 2
Inter Boundary Continuity 4 | InterBoundaryContinuity4 | Inter Boundary Continuity 4 |  | Integer | 0 - 2 | 0 - 2
Inter Boundary Continuity 5 | InterBoundaryContinuity5 | Inter Boundary Continuity 5 |  | Integer | 0 - 2 | 0 - 2
Position Tolerance | PositionTolerance | Position Tolerance |  | Double | 0.0 - 1.0 | 0.0 - 1.0
Tangent Tolerance | TangentTolerance | Tangent Tolerance |  | Double | 0.0 - 1.0 | 0.0 - 1.0

Autodesk Softimage v7.5