ufoProcessRasterInDefine

    void ufoProcessRasterInDefine(
       ufoProcess process_instance,
       int input_index,
       char *id,
       char *name,
       ufoCompComb suggested_components);

Refer to the following table for command descriptions:

Command | Description
    input_index
| index (0..number_inputs-1) of raster input
    id
| unique (within process) id of input with no spaces
    name
| user interface title of input
    suggested_components
| suggested working pixel components
    ufoCompComb
    ufoAnyCompComb
| expects any pixel type
    ufoRGBCompComb
| expects RGB pixel type
    ufoRGBACompComb
| expects RGBA pixel type
    ufoACompComb
| expects A pixel type

ufoProcessRasterInDefine defines one of the (0..number_inputs-1) raster inputs as set in the ufoProcessCreate function call.

The suggested_components argument indicates which component combination of the raster the UFO process expects to work on. This does not force the pixel type of raster supplied when rendering; for this use ufoProcesSetPixelTypeCombinations.

ufoProcessRasterInDefine must be called within ufoProcessDefine for each raster input.

Autodesk Softimage v7.5