P

PassThroughNode

Introduced

7.0

UI Location

• Execution

Description

Outputs the input data without any modification. This node is useful when one needs to branch out one compound input port to drive many ports inside the compound. A Pass Through node is automatically created when reusing an existing exposed port to drive another node port that is in the compound (when editing a compound, click and drag from an already existing exposed input port to a new port of the same type.

Port Description

Inputs

Group ID | Instance s | Port Name | Connection Info | Description
0 | 1 | in | • Type: siICENodeDataAny • Structure: siICENodeStructureAny • Context: siICENodeContextAny | The input values or execution to pass through.

Outputs

Port Name | Connection Info | Description
out | • Type: siICENodeDataAny • Structure: siICENodeStructureAny • Context: siICENodeContextAny | The same values or execution connected to the input port.

Restrictions

• These types must match: in, out

• These structures must match: in, out

• These contexts must match: in, out

See Also

ExecuteNode | FilterNode | FirstValidNode | IfNode
RepeatNode | SelectCaseNode | WhileNode |

Autodesk Softimage v7.5