Link Parameter Functions

l_fcv(<parameter>)

The Linked Parameter (l_fcv) token defines a link relationship between two parameters. The <parameter> argument represents a parameter name.

| Using this function nests an extra Parameter containing an FCurve object (which you can get via the Parameter.Source property) under the Expression object.

l_interp(<param1> <param2> ...)

The Multi-linked Parameters (l_interp) token defines a link relationship from many parameters to one.

| Using this function nests an extra Property (Interpolation) under the Expression object containing the sigma Parameter which determines the falloff for the interpolation between multiple inputs.

l_interpOri((rotx, roty, rotz)<param>)

The Orientation-linked Parameters (l_interpOri) token defines a link relationship between an object's orientation and a parameter.

| Using this function nests an extra Property (Interpolation) under the Expression object containing the sigma Parameter which determines the falloff for the interpolation between multiple inputs.

Autodesk Softimage v7.5