ColorToRGBANode

Introduced

7.0

UI Location

• Color

• Conversion

Description

Outputs the red, green, blue and alpha components of the input color space.

Note: The input alpha component has no effect on the conversion. The resulting alpha component equals the alpha component of the specified input color.

Port Description

Inputs

Group ID | Instance s | Port Name | Connection Info | Description
0 | 1 | color | • Type: siICENodeDataColor4 • Structure: siICENodeStructureAny • Context: siICENodeContextAny | The color to convert.

Outputs

Port Name | Connection Info | Description
red | • Type: siICENodeDataFloat • Structure: siICENodeStructureAny • Context: siICENodeContextAny | The red component of the input color.
green | • Type: siICENodeDataFloat • Structure: siICENodeStructureAny • Context: siICENodeContextAny | The green component of the input color.
blue | • Type: siICENodeDataFloat • Structure: siICENodeStructureAny • Context: siICENodeContextAny | The blue component of the input color.
alpha | • Type: siICENodeDataFloat • Structure: siICENodeStructureAny • Context: siICENodeContextAny | The alpha component of the input color.

Restrictions

• These structures must match: color, red, green, blue, alpha

• These contexts must match: color, red, green, blue, alpha

See Also

AddColorNode | BlendColorNode | ColorNode | ColorToBrightnessNode
ColorToGrayscaleNode | ColorToHLSANode | ColorToHSVANode | GradientNode
HLSAToColorNode | HSVAToColorNode | MultiplyColorByScalarNode | RGBAToColorNode
SubtractColorNode |  |  |

Autodesk Softimage v7.5