## mergesrf

Merge Surfaces

Type:
  XSI Object

Spdl File:
  %XSI_HOME%\Application\spdl\mergesrf.spdl

Parameter Name | Scriptname | Description | Valid Values | Data Type | Range | UI Range
--- | --- | --- | --- | --- | --- | ---
Surface 1 | boundsrf1 | Boundary for surface 1 (start boundary) |
0 | Min U Boundary (Red)
1 | Max V Boundary
2 | Max U Boundary
3 | Min V Boundary (Green)
| Integer |  |
Surface 2 | boundsrf2 | Boundary for surface 2 (end boundary) |
0 | Min U Boundary (Red)
1 | Max V Boundary
2 | Max U Boundary
3 | Min V Boundary (Green)
| Integer |  |
Continuity | cont | Continuity (C0, C1 or C2) |
0 | Position (C0)
1 | Tangent (C1)
2 | Curvature (C2)
| Integer |  |
Seam | seam | Seam to which the merge should take place |
0 | First Surface
1 | Second Surface
2 | Average
3 | Curve
| Integer |  |
Modify Tangent | modifytan | Surface to which tangent should be modified |
0 | First Surface
1 | Second Surface
2 | Both Surfaces
| Integer |  |
Fix Boundary | boundfix | Fix Boundary |
0 | Mode 1
1 | Mode 2
2 | Mode 3
3 | Mode 4
| Integer |  |
Range | startrange | Range |  | Double | 0.0 - 1.0 | 0.0 - 1.0
Range | endrange | Range |  | Double | 0.0 - 1.0 | 0.0 - 1.0
Tangent Scale Factor | startscl | Tangent scale factor for surface 1 |  | Double | 0.0 - 1.0 | 0.0 - 1.0
Tangent Scale Factor | endscl | Tangent scale factor for surface 2 |  | Double | 0.0 - 1.0 | 0.0 - 1.0
Shape Factor | shpfactor | Shape Factor |  | Double | 0.0 - 1.0 | 0.0 - 1.0
Tolerance | tol | Cleaning tolerance |  | Double | 0.0 - 10.0 | 0.0 - 2.0

Autodesk Softimage v7.5