ConnectICENodes

Introduced

7.0

Description

Connects two nodes through the specified ports (components).

Scripting Syntax

    ConnectICENodes( [InputPort], [OutputPort] )

Parameters

Parameter | Type | Description
InputPort | String | Input port on the target node (ICENodeInputPort). Default Value: If not specified, the user is prompted to select a target.
OutputPort | String | Output port on the source node (ICENodeOutputPort). Default Value: If not specified, the user is prompted to select a source.

See Also

AddAttributeToSetDataICENode | AddICECompoundNode | AddExposedParamToICECompoundNode | AddICENode
AddNodeToICECompoundNode | CleanDisconnectedICENodes | CreateICECompoundNode | DisconnectICENodePort
EditExposedParamInICECompoundNode | ExplodeICECompoundNode | RemoveAttributeFromSetDataICENode | RemoveExposedParamFromICECompoundNode
RemoveNodeFromICECompoundNode |  |  |

Autodesk Softimage v7.5