## blendsrf

Blend Surfaces

Type:
  XSI Object

Spdl File:
  %XSI_HOME%\Application\spdl\blendsrfop.spdl

Parameter Name | Scriptname | Description | Valid Values | Data Type | Range | UI Range
--- | --- | --- | --- | --- | --- | ---
Use Surface Curve | srfcrvsrf1 | Use surface curve on surface 1 |  | Bool |  |
Use Surface Curve | srfcrvsrf2 | Use surface curve on surface 2 |  | Bool |  |
Surface 1 | boundsrf1 | Boundary for surface 1 (start boundary) |
0 | Min U Boundary (Red)
1 | Max V Boundary
2 | Max U Boundary
3 | Min V Boundary (Green)
| Integer |  |
Surface 2 | boundsrf2 | Boundary for surface 2 (end boundary) |
0 | Min U Boundary (Red)
1 | Max V Boundary
2 | Max U Boundary
3 | Min V Boundary (Green)
| Integer |  |
Continuity | startcont | Continuity for surface 1 |
0 | Position (C0)
1 | Tangent (C1)
2 | Curvature (C2)
| Integer |  |
Continuity | endcont | Continuity for surface 2 |
0 | Position (C0)
1 | Tangent (C1)
2 | Curvature (C2)
| Integer |  |
Tangent Scale Factor | startscl | Tangent scale factor for surface 1 |  | Double | -10.0 - 10.0 | -1.0 - 1.0
Tangent Scale Factor | endscl | Tangent scale factor for surface 2 |  | Double | -10.0 - 10.0 | -1.0 - 1.0
Position Tolerance | postol | Position Tolerance |  | Double | 0.0 - 2.0 | 0.0 - 2.0
Angular Tolerance | angtol | Angular Tolerance |  | Double | 0.0 - 2.0 | 0.0 - 2.0
Tangent Direction Match | starttandir | Tangent direction match at start surface |  | Bool |  |
Tangent Direction Match | endtandir | Tangent direction match at end surface |  | Bool |  |
Position | srfcrvindex1 | Position (index) of the surface curve on surface 1 |  | Integer | 0 - 10 | 0 - 10
Position | srfcrvindex2 | Position (index) of the surface curve on surface 2 |  | Integer | 0 - 10 | 0 - 10
Shift | shiftvalsrf1 | Shift value for surface 1 |  | Double | 0.0 - 1.0 | 0.0 - 1.0
Shift | shiftvalsrf2 | Shift value for surface 2 |  | Double | 0.0 - 1.0 | 0.0 - 1.0

Autodesk Softimage v7.5