Interoperability Tutorials > Using Autodesk Revit >
Preparing the Scene in Revit

In this lesson, you use Revit to adjust some settings before enhancing the scene in 3ds Max Design.

To complete this lesson, you must have Revit installed on your workstation. If you do not have Revit installed, proceed directly to the next lesson, Linking a 3ds Max Design Scene to the FBX File.

Set up the lesson:

1. Open the Revit application. Click (Open). Navigate to the 3ds Max Design tutorial project folder \import\Revit_files. Highlight beachhouse.rvt and click Open.
   NoteIf you are using a version of Revit that is earlier than Revit 2012, you should use an appropriate earlier version of this tutorial. You can find earlier tutorials at this Web page. If you use an earlier version of this tutorial, be sure to download the sample files appropriate to that version: Extract them to a project folder that is distinct from the one you use for the 3ds Max Design tutorials.

   The beachhouse.rvt project features the model of a bungalow situated on a beach. In the procedure that follows, you will use options in Revit to change the model’s roof material, in preparation for exporting the scene.

   NoteEven though you can modify materials in 3ds Max Design, it is a good idea to make your changes in Revit if this is the application you are the most comfortable using.
2. Use the SteeringWheels controls to zoom in on the beach house.

Change the roof material in Revit:

1. Click to select the roof object, then on the ribbon, click (Type Properties).

   Revit opens the Type Properties dialog.

2. On the Type Properties dialog Type Parameters group Construction rollout Structure item, click Edit.

   Revit opens the Edit Assembly dialog.

3. On the Edit Assembly dialog, click << Preview.

   Revit displays a panel to the left, showing a detailed cross-section of the roof.

4. In the Layers group Material column, click the top item in the list, Roofing - Asphalt.

   After you click the Roofing - Asphalt entry, a browser button appears. Click this button.

   Revit opens a Materials dialog.

5. On the Materials dialog, click the Appearance tab to display a thumbnail of the roof shingle material.
6. In the Materials tab at the left, scroll down in the list of materials and choose Roofing - Slate.
   NoteIf this material is not available on your system, choose an alternate material.
7. Click OK on all the open dialogs to exit the material edit controls.

   The texture and mapping coordinates of your selected material will be properly transferred to 3ds Max Design, with no further intervention required on your part.

Check light-object properties in Revit:

Like materials, all light-object properties in the Revit scene are accurately transferred to 3ds Max Design. Therefore, it is best to make sure that the lights you have in the current scene possess the properties you want to use in 3ds Max Design.

1. In the Project Browser panel at the left, under Views Ceiling Plans, double-click Level 1.

   Revit displays the plan of the ceiling.

2. Zoom in to get a closer view of the ceiling plan for the main part of the house.

   There are seven ceiling lights inside the house, and three outside on the porch.

3. Click to select any ceiling light object in the scene.

   Revit displays a description of the light object in the Properties panel to the left.

4. On the Properties panel, click Edit Type.

   Revit opens a Type Properties dialog.

5. On the Type Properties dialog Type Parameters group, scroll down to the Photometrics rollout and review the parameters displayed.

   These values, particularly Initial Intensity and Color, will affect the rendered result in 3ds Max Design, so be sure these parameters contain the result you are looking for. (You can later update these values in 3ds Max Design, if you need to.)

6. Click the Initial Intensity button to view more detail on light intensity.
   Note 3ds Max Design uses Lumens rather than Watts to measure light intensity. When a Revit scene is imported into 3ds Max Design, all wattage is converted into Lumens, but intensity of the light object is not affected.
7. Click OK to exit the dialogs.
8. Back in the Level 1 view, click to select the Pendant Light object. This is the light at the lower right of the ceiling plan, in the dining area.
9. On the Properties panel, click Edit Type to open the Type Properties dialog.
10. Review the Photometric properties as you did for the ceiling light object.
11. Click OK to exit the dialogs.

Create a camera:

By default, the 3D view in Revit uses an isometric perspective, but an FBX file must contain a single camera view: This view is the Revit camera that is active at the moment of export. Therefore, you must create at least one camera view in Revit before you export the scene. In this procedure, you create a camera for an exterior viewpoint.

NoteAlthough you can create multiple cameras in Revit, you can export only one camera view to the FBX file. Cameras that are not active are not exported.

1. In the Project Browser panel, navigate to Views Floor Plans and double-click Level 1.
2. Zoom so you have a view of the house and the area around it.
3. On the ribbon, go to the View tab.
4. On the Create panel, open the 3D View drop-down list, and choose Camera.
5. Place the camera by clicking below the reference object at the left of the scene, then click a point along the front wall of the house, to the left of the double doors.

   Revit creates a camera view. This is the view you will initially use to render your image in 3ds Max Design. It also changes the ribbon to show the Modify | Cameras tab.

6. On the Properties panel at the left, in the Identity Data rollout View Name field, change the name of the camera to Exterior, then click Apply (or press Enter).
7. Also on the Properties panel, scroll down to the Extents rollout. Turn off Far Clip Active.

   After a pause, the view shows hills in the distance.

   TipIf the hills in the distance don't appear interactively, click Apply.

   With Far Clip Active turned off, the camera is able to detect the scene terrain beyond the bungalow model. As with light and material properties, you can also modify clipping parameters in 3ds Max Design if you need to.

   Camera view with clipping turned off, showing scene background

   TipIf you want to adjust how the house is framed in the camera view, use the SteeringWheels Look and Walk tools to move the camera.

Set up rendering and the sun position:

1. Below the view, click (Show Rendering Dialog).

   Revit opens a Rendering dialog.

   Most of the rendering values do not need to be changed, since the actual rendering of the scene will take place in 3ds Max Design. The Scheme setting in the Lighting group is one possible exception.

   If you choose Exterior: Sun Only from the Lighting group Scheme drop-down list, then in the 3ds Max Design scene only the Daylight system will be turned on and all the man-made light objects will be turned off. Conversely, if you choose Interior: Artificial Only, only the interior man-made light objects will be used in the scene and the Daylight system will be turned off.

2. For this tutorial, we do not want to use the interior lights yet, so leave Scheme set to the default value, Exterior: Sun Only. (You will turn the man-made lights back on in 3ds Max Design, when you need them.)
3. For the Lighting group Sun Setting, click the sun location button.

   Revit opens a Sun Settings dialog, where you will set the geographic location and time of day for the position of the sun created by the daylight system.

4. In the Solar Study group, click to choose Still.

   (The Single Day and Multi-Day tabs let you choose presets that animate the position of the sun over the course of one or more days.)

   Keep the default location of Boston, Massachusetts, because we imagine the house to be on Cape Cod, which is only slightly south of the city.

5. In the Settings group Date field, change the month to 5 and the day of the month to 10.
6. Change the time to 3:17 PM.
7. In the Settings group, click Save Settings.

   Revit opens a Name dialog for the new preset.

8. On the Name dialog, type East Coast, then click OK.

   This name is appropriate because you want the Daylight system to show the actual sun position at Cape Cod in mid-afternoon.

   The name of the preset now appears in the list in the Presets group.

9. Click OK to close the Sun Settings dialog.
10. Close the Rendering dialog.

    Now you are ready to export the scene file to FBX format.

Export the scene:

To export from Revit to the FBX format, you need to be in a 3D view, such as the Exterior camera view you have just created.

1. Open the Application menu and choose Export FBX.
   NoteAt this point, Revit might prompt you to save the project. You don’t need to save the project to proceed with this tutorial.
2. Revit opens an Export 3ds Max (FBX) dialog. In the File Name/Prefix field, change the name of the file to beachhouse. If you need to, navigate to the \import\Revit_files folder (not one of the subfolders), then click Save to export the scene.
3. Minimize Revit but don’t close it, as you will use it again later in this tutorial.

Next

Linking a 3ds Max Design Scene to the FBX File