Inputting and Outputting Media > Importing Media Files and Sequences > Media Files Import Preferences and Import History Options > RED-Only Preferences >

# Debayering Menu

Debayering box
  Select the level of quality required from the debayering algorithm. Higher resolutions are significantly more processing intensive.
  NoteThe debayering setting is the most resource-intensive setting. Try using the level of debayering the most appropriate for your work.
Bit Depth box
  Set the bit depth of the imported image. If you set Debayering > HDRx box to High Dynamic Range, HDRx footage is always imported as a 16-bit floating point clip, even if Bit Depth is set to 12bit Integer.
Detail box
  Select the level of detail extraction required.
Denoise box
  Select the level of noise reduction applied to the debayered clip.
OLPF Compensation box
  Select the level of Optical Low Pass Filter (OLPF) compensation to use. OLPF is a type of sharpening used to compensate for the optical anti-aliasing filter, which can induce softening of the image during recording.