Summary:

This part illustrates some of the overrides that can be applied to sheet metal features. Almost all of the sheet metal settings can be overridden on a per feature basis. For example, the upper flanges have round bend relief on one side and square relief on the other. These differences are also called out in the associated drawings.

The drawings (idw and dwg files) that have been created here show many new and modified annotations. The drawings show standard view projections, a shaded isometric view, detail views, and a view of the flatpattern. There are also examples of Hole Notes, Hole Tables, Bend Tables, Chamfer Notes, and the use of Bend Centerline formatting.