Importing and Exporting Media > Clip Input/Output Using a VTR > Audio Gain Adjustment Settings >

# Adjusting Audio Gain on Clip Output

To adjust the audio gain on output clip:

1. Enable the Fader Lock buttons (so that they are light grey) if you want to apply the identical value to pairs of audio channels.
2. Slide the faders to adjust the audio gain before you start processing. Use the All Audio button to monitor all the audio tracks that are output, regardless of what audio tracks the VTR records.
3. In the VTR Output module, enable Output All Audio.
4. Select or deselect channels for output by clicking the Channel Selection button for each channel as needed.
   NoteIn a multiple clip selection, channel selection is independent for each clip but the gain levels set with the faders are the same for all clips.
5. Process the clip.

   Selected channels are output.