Preferences >

# Audio Preferences

## Player

Monitor Sync box
  Indicates which monitor will have audio sync when you play back a clip (the broadcast monitor or the high-resolution monitor).

Broadcast Delay field
  Displays the number of frames (-30.00 to 30.00) to delay the audio signal when syncing to the broadcast monitor. Editable.

Hi-Res Delay field
  Displays the number of frames (-30.00 to 30.00) to delay the audio signal when syncing to the graphics monitor. Editable.

Auto Fade field
  Displays the amount of time (0 to 10 ms) that a fade is added to the start and end of each audio segment. Use this setting to avoid audible clicks between audio sources. Editable.

## Meters

Meter Range field
  Displays the overall scale for the fader meters. Editable.

Meter Green field
  Displays the green meter range. Editable.

Meter Yellow field
  Displays the yellow meter range. Editable.

Meter Step field
  Displays the step value for the meters. Enter a lower value to view a more detailed meter.

Meter Units box
  Select whether the meters display digital or analog units.

## Tone

Audio Tone box
  Select the default audio tone.

Reference Level field
  Displays the reference level for custom audio tones. Editable.

## Tracks

Consider Audio Head/Tail button
  Enable to include audio that extends before or after video when exporting movie files.

Supported Playback Tracks field
  Displays the number of playback tracks supported by your sound card. Non-editable.

Supported I/O Tracks field
  Displays the number of I/O tracks supported by your sound card. Non-editable.

Supported Audio Monitoring Field
  Displays the audio monitoring option supported by your sound card. Non-editable.

## Outputs

Output Source field
  Displays all current outputs. Non-editable.

Output Sampling Rate field
  Displays the current output sampling rate. Non-editable.