## output_format

Output Format Preferences

Type:
  XSI Object

Spdl File:
  %XSI_HOME%\Application\spdl\C3DPrefsOutputFormat.spdl

Parameter Name | Scriptname | Description | Valid Values | Data Type | Range | UI Range
--- | --- | --- | --- | --- | --- | ---
Preset | preset |  |  | Integer | Min - Max |
vert_spacing | vert_spacing |  |  | String |  |
Picture Standard | picture_standard |  |
0 | Custom
1 | Cine 35 1.37/1
2 | Cine 35 1.66/1
3 | Cine 35 1.85/1
19 | Cine 35 Vistavision
4 | Cine 70 Panavision
5 | Cine 70 Imax
20 | Cine 16
21 | Cine Super 16
6 | Slide 35 (24x36)
7 | Slide 6x6
8 | Slide 4"x5"/8"x10"
9 | NTSC D1 4/3 720x486
12 | NTSC D1 16/9 720x486
22 | NTSC DV 720x480
10 | PAL D1 4/3 720x576
13 | PAL D1 16/9 720x576
14 | HDTV 480 640x480
15 | HDTV 480 4/3 704x480
16 | HDTV 480 16/9 704x480
17 | HDTV 720 16/9 1280x720
11 | HDTV 1035 16/9 1920X1035
18 | HDTV 1080 16/9 1920x1080
| Integer | 0 - Max |
Picture Ratio | picture_ratio |  |  | Double | 0.0 - Max | 0.0 - 3.0
Resolution X | ir_xres |  |  | Integer | 1 - Max | 1 - 2048
Resolution Y | ir_yres |  |  | Integer | 1 - Max | 1 - 2048
Pixel Ratio | ir_pixel_ratio |  |  | Double | 0.0 - Max | 0.0 - 2.0
Maintain Picture Ratio | ir_inverse_ratio |  |  | Bool |  |
Pixel Ratio | roto_pixel_ratio |  |  | Double | 0.0 - Max | 0.0 - 2.0
Use Camera Pixel Ratio | roto_use_pixel_ratio |  |  | Bool |  |
Update PlayControl | update_playcontrol |  |  | Bool |  |
Frame Step | frame_step |  |  | Integer | 1 - Max |
Frame Format | frame_format |  |
10 | NTSC (29.97 fps)
8 | PAL (25 fps)
7 | Film (24 fps)
19 | 30 fps
13 | 23.976 fps
25 | 59.94 fps
11 | Custom framerate
| Integer |  |
Frame Rate | frame_rate |  |  | Double | 0.1 - Max | 0.1 - 100.0
Enable Fields | field_enable |  |  | Bool |  |
Interleave | field_interleave |  |  | Bool |  |
Field Order | field_order |  |
0 | Lower Field First / Even (NTSC)
1 | Upper Field First / Odd (PAL and HD Formats)
| Integer | 0 - 1 |
preset_to_delete | preset_to_delete |  |  | Integer | Min - Max |

Autodesk Softimage v7.5