AlignedAxisConstrai nt

Object Hierarchy

Inheritance

    SIObject
       ProjectItem
           Property
              Constraint
                  AlignedAxisConstraint

Description

The AlignedAxisConstraint object represents a AxisAligned constraint e.g. Direction, Position constraint.

Methods

AddCustomOp | AddScriptedOp | AddScriptedOpFromFile | AnimatedParameters2
BelongsTo | EvaluateAt | GetICEAttributeFromName | IsA
IsAnimated2 | IsClassOf | IsEqualTo | IsKindOf
IsLocked | IsSelected | LockOwners | SetAsSelected
SetCapabilityFlag | SetLock | TaggedParameters | UnSetLock

Properties

Application | Branch | BranchFlag | Capabilities
Categories | Constrained | Constraining | Families
FullName | Help | ICEAttributes | LockLevel
LockMasters | LockType | Model | Name
NestedObjects | ObjectID | Origin | OriginPath
Owners | Parameters | Parent | Parent3DObject
PPGLayout | Selected | Singleton | Type
UpVectorReference | UpVectorReference |  |

Examples

VBScript Example

       'The following code illustrates how to create an axis aligned constraint
       ' and set its upvector reference.

    set oRoot = Application.ActiveProject.ActiveScene.Root
    set oNull = oRoot.AddNull
    '    set oNull.Kinematics.Local.Translate -6.546, 4.815, -0.482
    set oNull2 = oRoot.AddNull
    '    set oNull2.Kinematics.Local.Translate 6.624, 5.907, -0.591
    set oGrid = oRoot.AddGeometry("Grid","MeshSurface")

    set oDirectionCns = oGrid.Kinematics.AddConstraint("Direction", oNull )
    set oDirectionCns.UpVectorReference = oNull2

See Also

Kinematics | Kinematics.AddConstraint

Autodesk Softimage v7.5