## extrusion

Extrude a curve to create a surface

Type:
  XSI Object

Spdl File:
  %XSI_HOME%\Application\spdl\extrusionAxisOp.spdl

Parameter Name | Scriptname | Description | Valid Values | Data Type | Range | UI Range
--- | --- | --- | --- | --- | --- | ---
Close in U | closeu | Close the resulting surface in U |  | Bool |  |
Close in V | closev | Close the resulting surface in U |  | Bool |  |
Start Position | startpos | Start position of the extrusion |  | Double | Min - Max | 0.0 - 100.0
Length | length | Length of the extrusion |  | Double | Min - Max | 0.0 - 100.0
Snap to Profile | snapprof | Move the path of the extrusion to the profile curve |  | Bool |  |
From Center. | fromcenter | Percentage from center to first point of profile. |  | Double | -1000.0 - 1000.0 | -100.0 - 100.0
Extrude Along X | alongx | Extrude along the X axis |  | Bool |  |
Extrude Along Y | alongy | Extrude along the Y axis |  | Bool |  |
Extrude Along Z | alongz | Extrude along the Z axis |  | Bool |  |
Local Axis | localaxis | Extrude Along Local Axis Instead of Global Axis |  | Bool |  |

Autodesk Softimage v7.5