ufoProcessRasterOutDefine

    void ufoProcessRasterOutDefine(
       ufoProcess process_instance,
       int output_index,
       char *id,
       char *name,
       ufoCompComb suggested_components);

Refer to the following table for command descriptions:

Command | Description
    output_index
| index (0..number_outputs-1) of raster output
    id
| unique (within process) id of output with no spaces
    name
| user interface title of output
    suggested_components
| suggested working pixel components
    ufoCompComb
    ufoAnyCompComb
| expects any pixel type
    ufoRGBCompComb
| expects RGB pixel type
    ufoRGBACompComb
| expects RGBA pixel type
    ufoACompComb
| expects A (alpha) pixel type

ufoProcessRasterOutDefine define one of the (0..number_outputs-1) raster outputs as set in the ufoProcessCreate function call.

The suggested_components argument indicates which component combination of the raster the UFO process expects to work on. This does not force the pixel type of raster supplied when rendering; for this use ufoProcesSetPixelTypeCombinations.

ufoProcessRasterOutDefine must be called within ufoProcessDefine for each raster output.

Autodesk Softimage v7.5