Basic Data Types

Several types are available in the Crosswalk SDK for cross-platform compatibility. It is highly recommended that you use them as much as possible to ensure that the code is portable to other platforms.

This is the mapping of Crosswalk SDK types:

Crosswalk SDK Types | C types
SI_Bool | unsigned short
SI_Byte | char
SI_Ubyte | unsigned char
SI_Short | short
SI_Ushort | unsigned short
SI_Int | int
SI_Uint | unsigned int
SI_Float | float
SI_Double | double
SI_Long | long
SI_Void | void
SI_Ulong | unsigned long

Autodesk Softimage v7.5